|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **identifier** | **URI** | **OID (for non-FHIR systems)** | **Type** | **Comment** |
| URIs ([W3C](http://www.w3.org/)): when the identifier is a URI | urn:ietf:rfc:3986 | 2.16.840.1.113883.4.873 |  | As defined by [RFC 3986](http://www.ietf.org/rfc/rfc3986.txt) (with many schemes defined in many RFCs). For OIDs and UUIDs, use the URN form ([urn:oid:](http://www.ietf.org/rfc/rfc3001.txt) (note: lowercase) and [urn:uuid:](http://www.ietf.org/rfc/rfc4122.txt) |
| [DICOM Unique Id](https://www.dicomstandard.org/) | urn:dicom:uid |  |  | An OID issued under DICOM OID rules. DICOM OIDs are represented as plain OIDs, with a prefix of "urn:oid:" |
| [United States Social Security Number](http://www.ssa.gov/) | http://hl7.org/fhir/sid/us-ssn | 2.16.840.1.113883.4.1 | [SB](http://build.fhir.org/v2/0203/index.html#SB) (US) | The SSN is represented in resources with dashes removed |
| [United States Medicare Number](https://www.medicare.gov/) | http://hl7.org/fhir/sid/us-medicare | 2.16.840.1.113883.4.572 | [SB](http://build.fhir.org/v2/0203/index.html#SB) (US) | Medicare Numbers (HIC or HICN) are represented without any spaces or dashes |
| [Medicare Beneficiary Identifier (United States)](https://www.medicare.gov/) | http://hl7.org/fhir/sid/us-mbi | 2.16.840.1.113883.4.927 | [SB](http://build.fhir.org/v2/0203/index.html#SB) (US) | Medicare Beneficiary Identifiers are represented without any spaces or dashes |
| [United States National Provider Identifier](http://www.cms.gov/) | http://hl7.org/fhir/sid/us-npi | 2.16.840.1.113883.4.6 | [PRN](http://build.fhir.org/v2/0203/index.html#PRN) (US) |  |
| [Global Trade Item Number (GTIN)](http://www.gs1.org/) | https://www.gs1.org/gtin | 1.3.160 |  | Note: GTINs may be used in both [Codes](http://build.fhir.org/datatypes.html#Coding) and [Identifiers](http://build.fhir.org/datatypes.html#Identifier) |
| Bluetooth address | http://hl7.org/fhir/sid/eui-48/bluetooth |  |  | The Bluetooth address of devices communicating using the Bluetooth transport protocol |
| Ethernet address | http://hl7.org/fhir/sid/eui-48/ethernet |  |  | The ethernet MAC address of devices communicating over the ethernet |
| ZigBee address | http://hl7.org/fhir/sid/eui-64/zigbee |  |  | The ZigBee address of devices communicating using the ZigBee transport protocol |
| USB address | http://hl7.org/fhir/sid/usb |  |  | The USB PID and VID values of devices communicating using USB. |